This document lists the updates and corrections for the firmware installed the Lovibond PFXi Series of instruments.

V3.7

* Corrected translation spelling.
* Added calculation of Gardner colour scale for the scale region 0 to 1
* Added calculation of ASTM Color scale for the region 0 to 0.5

V3.91

* Implemented Hess Ives Color Scale
* Corrected Printout for EP colour Scale

V4.0

* Corrected Issues for communicating with the Windows Host Software

V4.02

* Yellowness Index corrected to show 1 decimal point

V4.2

* Company External IP address changed for RCMSI communication

4.4

* Improved Platinum Cobalt correlation in PFXi195 for values above 400 Platinum cobalt

4.5

* Improvement to PFXi195 Platinum Cobalt calibration (Firmware Not released)

4.6

* Recalibration to PFXi195 for Platinum Cobalt: Checked against internal and external standards.